®

Value-Add Capabilities

Steel Coil Value-Added Processing Solutions

steelscape.com

Value-Add

Steelscape offers a range of value-add processing services designed to deliver material ready for downstream production. By reducing additional handling, trimming, and processing requirements, these capabilities help improve efficiency while supporting consistent quality and dimensional accuracy.
Embossing

A non-directional stucco embossed pattern adds texture and depth to metal products. Available on bare and painted substrates, embossed products are commonly used in architectural siding, and cold storage applications. Manufactured in Rancho Cucamonga, CA.

Cut-To-Length

Cut-to-length converts painted and coated coils into precise flat sheets or plates. This process supports consistent dimensions while reducing the need for downstream handling or additional
cutting. It provides fabrication-ready sheets tailored to project-specific requirements. Manufactured in Kalama, WA
Slitter

Slitting converts master coils into precise narrower widths. This process supports consistent edge quality and dimensional accuracy while reducing the need for downstream trimming and processing. Manufactured in Kalama, WA and Rancho Cucamonga, CA.

®

Value-Add Capabilities

888-553-5521

©2026 Steelscape, LLC All rights reserved. TruZinc® is a registered trademark of Steelscape, LLC. ZINCALUME® is a registered trademark of BlueScope Steel Ltd. SPS144 0726 web

steelscape.com

VALUE-ADD CAPABILITIES
Embossing	Cut-to-Length Sheet

* If outside of this thickness and wider than 48.5″, inquire with your Steelscape Representative.
** Grade/hardness restrictions may apply to some substrates. Cannot process Grade 80 steel. Grade 50 above 0.0236″, inquire with your Steelscape Representative.
*** Embossed material will collapse if packaged longitudinally.

Vertical Only***

Available

Required

OD 64″/ID 20″

20”

TruZinc® (HDG), ZINCALUME® (Galvalume), CRS, ALUM**

. 007″ up to .01″ thick

23.937″ – 48.5″ Steel 18″ – 48.5″ Aluminum

0.0180″ – 0.0296″ Steel* 0.0320″ – 0.040″ Aluminum

12,500 #

30,000 #

Non-Directional Stucco

Rancho Cucamonga

Pattern
Max Entry Coil Wt Max Output Coil Wt
Thickness (T)

Width

Depth Substrates Entry OD/ID Delivery OD/ID Cores
Reverse Wrap
Packaging

* Maximum thickness is limited for fluorocarbon paint systems due to concern with scratching top surface upon stacking. Inquire with your Steelscape representative for painted product greater than 0.0236″ ordered thickness.
** Standard width is 48″, it can be made available in any width up to 60″.

48″ (-0.25″/+0.375″)

24″ with skid

84″/20″ +/- 0.5″

120″ (up to 150″ – trial only)

36”

15,000 #

12″ – 60″

0.010″ – 0.050″ Bare*
0.0101 – 0.030″ Painted*

65 KSI (90 KSI up to .030″ thick)

50 KSI

60,000 #

Kalama

Max Entry Coil Weight Max Shear Strength Max Yield Strength
Thickness (T)

Width
Max Pallet Weight Min. Cut Length Max. Cut Length Entry OD/ID
Min. Stack Height
Strippable Film**

Slitting

Facility	Kalama	Rancho Cucamonga	
Max Entry Coil Weight	55,000 #	20,000 #	
Max Delivery Weight	55,000 #	20,000 #*	
Thickness (T)	0.010″ – 0.050″	0.011″ – 0.046″ Steel 0.032″ – 0.063″ Aluminum	
Width	16″ – 52″	12″ – 52″	
Max. Number Mults	24	20 if .025″<T<.050″
40 if T<.025″	
Maximum # sizes per setup	Depends on knives & size of mults	Depends on knives & size of mults	
Minimum Slit Width (W)**	2.00″	4.00″	
Entry OD/ID***	79″ max/20″	64″ max/20″	
Delivery OD/ID	79″ max/20″	64″ max/20″	
Cores****	W > 10″, T < 0.030″	W > 10″	
Min. Slit Drop	0.375″	0.375″	
* If vertical, skidded maximum weight is 12,500#.
** For smaller widths inquire with your Steelscape Representative.
*** OD max depends on number of mults and crown in the coil.
**** Cores are “all or nothing” for the whole arm of mults (i.e. if one mult on the arm is less than 10″, then none of the mults on the arm can have cores).
Please inquire for cores < 10″ due to safety issues.