January 2025

RoHS/RoHS2/RoHS3 Compliance

Steelscape hereby certifies compliance with RoHS directive 2002/95/EC of January 27, 2003, EU Commission Decision 2005/618/EC of August 18, 2005, RoHS2 directive 2011/65/EU of January 2, 2013, and RoHS3 directive 2015/863 of July 22, 2019, that its TruZinc® and ZINCALUME® coated steel coils, when supplied as dry, no-chemical treatment/passivation, do not contain the below listed materials or substances in excess of the allowed thresholds.
All TruZinc® or ZINCALUME® coils ordered as dry, no chemical treatment/passivation, or with a RoHS compliant chemical treatment/passivation are RoHS, RoHS2 and RoHS3 compliant.

Material/Substance	Thresh.
Lvl.*	Yes	No	Notes, exceptions, etc.	
Cadmium (Cd)	0.01%		√		
Hexavalent Chromium (Cr+6)	0.1%		√		

Lead (Pb)	

0.1%		

√	Exceptions:
Lead in glass of electronic components
Lead in high melting temperature type solders (i.e. lead based solder alloys containing 85% by weight or more lead).
Lead in electronic ceramic parts	
Mercury (Hg)	0.1%		√		
Polybrominated Biphenyls (PBBs)	0.1%		√		
Polybrominated Diphenylethers (PBDEs)	0.1%		√		
Bis(2-ethylhexyl) phthalate (DEHP)	0.1%		√		
Butyl benzyl phthalate (BBP)	0.1%		√		
Dibutyl phthalate (DBP)	0.1%		√		
Diisobutyl phthalate	0.1%		√		
* Threshold Level, maximum concentration by weight in homogenous materials

Sincerely,
Michelle Vondran
Manager, Product Innovation & Technology Steelscape, LLC