January 2021

RoHS/RoHS2/RoHS3 Compliance

Steelscape hereby certifies compliance with RoHS Directive 2002/95/EC of January 27, 2003, 2005/618/EC of August 18, 2005, and RoHS2 amending directive of January 3, 2013, and RoHS3 amending directive of June 4, 2015 that its TruZinc® and ZINCALUME® coated steel coils, when supplied as dry, no-chemical treatment/passivation, do not contain the below listed materials or substances in excess of the allowed thresholds.

All TruZinc® or ZINCALUME® coils ordered as dry, no chemical treatment/passivation, or with a RoHS compliant chemical treatment/passivation are RoHS, RoHS2 and RoHS3 compliant.

Material/Substance	Thresh.
Lvl.*	Yes	No	Notes, exceptions, etc.	
Cadmium (Cd)	0.01%		√		
Hexavalent Chromium (Cr+6)	0.1%		√		

Lead (Pb)	

0.1%		

√	Exceptions:
Lead in glass of electronic components
Lead in high melting temperature type solders (i.e. lead based solder alloys containing 85% by weight or more lead).
Lead in electronic ceramic parts	
Mercury (Hg)	0.1%		√		
Polybrominated Biphenyls (PBBs)	0.1%		√		
Polybrominated Diphenylethers (PBDEs)	0.1%		√		
* Threshold Level, maximum concentration by weight in homogenous materials

Sincerely,

Michelle Vondran Technical Manager Steelscape

Steelscape, LLC | 222 West Kalama River Road, Kalama, WA 98625 (888) 553-5521 | www.steelscape.com