ZINCALUME®	ZINCALUME® Plus

ZINCALUME is a revolutionary metallic coated steel manufactured by Steelscape which provides unmatched durability and corrosion performance. Known by the trade name Galvalume®, this coating consists of an optimized 55% Aluminum-Zinc metallic coating over steel which offers up to a 60 year service life in exterior applications. ZINCALUME can be readily formed into a variety of end products and is commonly used as a material of choice for metal roof and wall products, enabling building designers to build once and roof once.
ZINCALUME is produced in accordance with the strict guidelines of the Zinc Aluminum Coaters Association which outlines
a scientifically perfected application process, maximizing corrosion performance and product quality. The reassurance offered by Steelscape’s ZINCALUME is supported by a limited 25 and a half year corrosion warranty.
Steelscape offers ZINCALUME bare, or in an endless array of colors, finishes and textures, providing ultimate design freedom. ZINCALUME steel is proudly produced in Steelscape’s Rancho Cucamonga California facility, which includes ZINCALUME coating and painting capabilities in the one location, facilitating exceptional product quality management and coating flexibility.

A clear odorless resin applied to ZINCALUME provides a surface that is easy to form and handle. ZINCALUME Plus forms an excellent finish for green building applications such as LEED and Living Building Challenge. ZINCALUME is Red List Free and offers a high three-year aged Solar Reflectance Index Value, meaning it reflects heat from the sun efficiently, reducing structure cooling costs.
The resin naturally and evenly dissipates over a period of 12-18 months (when left unpainted) without powdering, peeling, or cracking. This finish is optimized for product manufacturers as it minimizes the need for additional lubricants, resists scuff marks and fingerprints, allows for field painting without primer in most cases and protects the steel during storage and installation.

®

ZINCALUME® and ZINCALUME® Plus

	steelscape.com	

Benefits Overview
ZINCALUME
Superior corrosion performance
Smooth, uniform spangled finish
Long lasting service life (2-4x that of galvanized steel)
25 and half year limited warranty
Flexibility to be painted in a wide range of colors and finishes
Superior quality and consistency from Steelscape’s ZAC licensed, advanced application process

Additional Benefits to ZINCALUME Plus
Performance Qualities

Distinctive visual appeal
Environmentally responsible
Excellent lubricating qualities, reducing or eliminating the need for additional lubricants and roll cleaning
Resists scuff marks and fingerprints
Minimizes wet stack storage stain
Developed so product formers can transition from bare to painted without downtime
Allows for easy field painting without primer in most cases (with water-based paints)

Max Input Coil Weight:	55,000 #	
Max Output Coil Weight:	44,000 #	
Thickness:	0.0120" – 0.0356" *	
Width:	26" – 50"	
Coatings:	Resin / Oil / Passivant (Std or RoHS) / Paint	
Entry OD / ID:	79" max / 20" +/- 0.25	
Delivery OD/ID:	76" max / 20" +/- 0.25	
Coatings:	AZ50, AZ55, AZ60 **	
Manufacturing Location:	Rancho Cucamonga, CA.	

©2024 Steelscape, LLC All rights reserved. ZINCALUME® is a registered trademark of BlueScope Steel Ltd. Galvalume® is a registered trademark of BIEC International Inc. SPS050 0424 web

888-553-5521	steelscape.com

®

ZINCALUME® and ZINCALUME® Plus

* 0.0300” thickness & greater is considered non-surface critical for some product grades & end-uses, both bare and painted. Inquire with a Steelscape Sales Representative for further review.
** For heavier coating weights inquire with a Steelscape Sales Representative.

Interested to find out more about the development and advantages of ZINCALUME?
Ask us about our Introduction to ZINCALUME educational course.

Want to see the color and design options available on ZINCALUME?
Visit Steelscape.com to request a product sample today.