THE ULTIMATE HIGH-PERFORMANCE MATERIAL FOR INVITING FOOD STORAGE ENVIRONMENTS	

®

TruzGuard

Fast-track the creation of durable, high performance walk-in-coolers and food storage products with TruzGuard coated steel. Featuring a proven stain and fingerprint resistant coating, TruzGuard steel protects surfaces from the unsightly effects of surface staining and marring.
Durable, easy to clean, and available in a range of versatile colors, TruzGuard helps create functional cooler environments that are inviting for end users. TruzGuard is independently certified by NSF International as complying with NSF/ANSI 51, which expedites product approval as it meets NSF/ANSI 2, 6, 7, 12 and 25. TruzGuard is the superior, yet economical solution for walk in cooler siding or other interior applications requiring a robust surface material.
Why TruzGuard?
Stain and fingerprint resistant
Durable TruZinc® galvanized steel base, certified from 0.0187" through 0.0296" thickness
NSF tested and certified
Easy to clean
Available in 6 elegant colors and optional non-directional stucco embossing

Aged Bronze Gloss
IDZGAB01

Pewter Gloss
IDZGPW01

White Gloss
IDZGWH01

Copper Gloss
IDZGCP01

Silver Gloss
IDZGSV01

Black Gloss
IDZGBK01

Note: TruzGuard coated metal NSF/ANSI 51 is for Splash Zone and Nonfood Zone.

NSF/ANSI 51 certified

TRUZGUARD®

888-553-5521

©2020 Steelscape, LLC All rights reserved. SPS104 0420 web

steelscape.com